|  |  |  |
| --- | --- | --- |
| **Function** | **ComBrick** | **Smarty** |
| **Tx message** | Send to Smarty or PC  Write HEX on Serial (if enabled, only if not connected to helper) | Send via RF  Write HEX on Serial (if enabled) |
| **Debug** | Send to PC (if enabled) | Send via RF (if enabled)  Write HEX on Serial |
|  |  |  |